{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":626,"n_cols":5,"rows_kept":626,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["零星维修改造项目分项清单"]
["序号","分项工程名称","单位","综合单价/（含税）","备 注"]
[]
["一","土建"]
[1.1,"土（石）方工程"]
["1.1.1","人工挖土方","m³",null,"基坑围护"]
["1.1.2","机械挖土方","m³",null,"基坑围护"]
["1.1.3","人工回填（松填）土方","m³"]
["1.1.4","机械回填（夯实）土方","m³"]
["1.1.5","小挖掘机","小时",null,"斗容量0.8m3以下"]
["1.1.6","大挖掘机","小时",null,"斗容量0.8m3及以上"]
["1.1.7","机械开挖、自卸式汽车配合厂内运土方","m³",null,"斗容量0.8m3以下"]
["1.1.8","人工装土、拖拉机厂内倒运土方","车",null,"0.8m3"]
["1.1.9","清运建筑垃圾","m³",null,"场内运输"]
["1.1.10","清运建筑垃圾","m³",null,"外运"]
["1.1.11","场地平整","㎡",null,"推土机推土平整"]
["1.1.12","场地平整、碾压","㎡",null,"压路机15T以内，碾压遍数不少于纵横各6遍"]
["1.1.13","挖机场地平整","㎡",null,"绿化带或其它用推土机无法平整区"]
["1.1.14","钢管支架彩条布围护","㎡",null,"钢管支架间距2米，钢管水平横杆间距1米，围护墙高2米"]
["1.1.15","钢管支架彩钢板围护","㎡",null,"钢管支架间距2米，钢管水平横杆间距1米，围护墙高2米，板厚0.5mm"]
["1.1.16","拆除240mm厚砖砌体","㎡",null,"含双面粉刷层与垃圾清运费用"]
["1.1.17","砖砌体1：2水泥砂浆粉铲除20mm厚","㎡",null,"垃圾清运"]
["1.1.18","天棚水泥砂浆粉刷层铲除","㎡",null,"垃圾清运"]
["1.1.19","空心砖砌体240mm厚砖砌体","m³",null,"空心砖，海螺牌水泥"]
["1.1.20","实心砖砌体240mm厚砖砌体","m³",null,"水泥标准砖"]
["1.1.21","加气块砖砌体240mm砌体","m³",null,"加气混凝土砌块，海螺牌水泥"]
["1.1.22","砖砌体1：2水泥砂浆粉刷20mm厚","㎡",null,"中粗沙、海螺牌水泥"]
["1.1.23","胶水和水泥掺合粉刷","㎡",null,"含材料、人工"]
["1.1.24","240mm厚墙面开洞≤300mm","个",null,"含恢复"]
["1.1.25","1.2～3.6m脚手架","㎡",null,"含材料、人工"]
["1.1.26","人工破除砼道路","m³",null,"含材料、人工"]
["1.1.27","小型挖掘机风镐破砼","小时",null,"斗容量0.8 m3以下"]
["1.1.28","碎石垫层摊铺","m³"]
["1.1.29","碎石垫层摊铺(利用原有）","m³",null,"厂内运输"]
["1.1.30","砼块垫层摊铺","m³",null,"砼块甲供、现场利用"]
["1.1.31","面包砖拆除","㎡",null,"含清运出厂，自行处理"]
["1.1.32","路侧石更换安装","m",null,"乙供材，含辅材，护帮砼乙供"]
["1.1.33","钢丝网围栏","m2",null,"含材料、人工"]
["1.1.34","钢丝网围墙钢管立柱更换","只",null,"含材料、人工"]
["1.1.35","刺绳","m",null,"含材料、人工"]
["1.1.36","有筋承插式涵管φ300×30×2000mm-Ⅱ敷设","m",null,"含材料、人工"]
["1.1.37","UPVC排水管DN50mm","m",null,"De50，华亚所有管材、管件均要求为国标,（余同）"]
["1.1.38","UPVC排水管DN75mm","m",null,"De75，华亚"]
["1.1.39","UPVC排水管DN 110mm","m",null,"De110，华亚"]
["1.1.40","UPVC排水45度弯头DN110mm","个",null,"De110，华亚"]
["1.1.41","UPVC排水直接DN50mm","个",null,"De50，华亚"]
["1.1.42","疏通Φ110mm雨污水管","m",null,"含垃圾清运"]
["1.1.43","清理雨水检查井（Ф700)","座",null,"综合各种深度、含垃圾清运"]
["1.1.44","排水沟清淤（300mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.1.45","疏通φ300mm污水管内油污","m",null,"含垃圾清运"]
["1.1.46","安装铸铁井圈井盖（Φ750，承载20t）","套",null,"井圈井盖乙供，含安装辅材"]
["1.1.47","甲供铸铁井圈井盖安装辅材","套"]
["1.1.48","砼地面开孔（Φ110mm，深300）","个",null,"含恢复、垃圾外运"]
["1.1.49","砼地面槽修复","m",null,"宽、深100mm以内"]
["1.1.50","砼地面开槽修复","m",null,"100mm×150mm"]
["1.1.51","C15商品砼人工浇筑地坪","m³",null,"含材料、人工"]
["1.1.52","C20商品砼人工浇筑地坪","m³",null,"含材料、人工"]
["1.1.53","C25商品砼人工浇筑地坪","m³",null,"含材料、人工"]
["1.1.54","C30商品砼人工浇筑地坪","m³",null,"含材料、人工"]
["1.1.55","C25地坪浇筑","m³",null,"砼自拌"]
["1.1.56","砼二次倒运","m³",null,"运距10米以内"]
["1.1.57","预埋件制安","kg",null,"马钢或国内大型钢厂产品"]
["1.1.58","钢构件制安","kg",null,"马钢或国内大型钢厂产品"]
["1.1.59","镀锌方管制作、安装","kg "]
["1.1.60","彩钢板墙面拆除","㎡",null,"拆除物归乙方所有"]
["1.1.61","彩钢板墙面安装","㎡",null,"含板材及辅材"]
["1.1.62","水管保温DN25","m",null,"橡塑保温"]
["1.1.63","制作彩钢雨棚","m2",null,"含材料、人工"]
["1.1.64","零星工程综合工日","工日",null,"小工"]
["1.1.65","零星工程综合工日","工日",null,"焊接等技术工种"]
["1.1.66","钢栏杆油漆（两遍）","m",null,"含除锈、一底二面"]
["1.1.67","地面油漆","m2",null,"黄色、白色油漆"]
["1.1.68","刷内墙涂料两面（含腻子）","㎡",null,"普通型"]
["1.1.69","外墙涂料二底二面","㎡"]
["1.1.70","外墙涂料二底二面","㎡",null,"普通型"]
["1.1.71","纸面石膏板吊顶","㎡",null,"含材料、人工"]
["1.1.72","轻钢龙骨纸面防潮石膏板隔墙单面石膏板","㎡",null,"含材料、人工"]
["1.1.73","墙面砖拆除后水泥粉刷","㎡",null,"含材料、人工"]
["1.1.74","地面砖拆除后水泥找平","㎡",null,"含材料、人工"]
["1.1.75","安装成品白榉木门","㎡",null,"含门套门锁不含铰链门吸门非实木门"]
["1.1.76","安装60型材推拉窗","㎡",null,"海螺型材、5mm单玻璃"]
["1.1.77","安装12mm厚木玻隔断钢化玻璃","㎡",null,"含材料、人工"]
["1.1.78","安装钢化玻璃门吊夹","只",null,"含材料、人工"]
["1.1.79","安装玻璃地弹门地锁","只",null,"含材料、人工"]
["1.1.80","PVC纱窗换纱","㎡",null,"含框料"]
["1.1.81","安装木门执手锁芯","把",null,"含材料、人工"]
["1.1.82","安装PVC门球形锁芯","把",null,"含材料、人工"]
["1.1.83","大挂锁","只",null,"含材料、人工"]
["1.1.84","小挂锁","只",null,"含材料、人工"]
["1.1.85","挂式小便斗","只",null,"含安装辅材"]
["1.1.86","小便冲水阀","只",null,"含安装辅材"]
["1.1.87","蹲便器","套",null,"含安装辅材"]
["1.1.88","大便冲水阀","只",null,"含安装辅材"]
["1.1.89","大便冲水管","根",null,"含安装辅材"]
["1.1.90","安装小便器按钮式冲洗阀","只",null,"含材料、人工"]
["1.1.91","大便器手柄式可调冲洗阀","套",null,"含材料、人工"]
["1.1.92","安装给水三角阀","只",null,"含材料、人工"]
["1.1.93","安装卫生间隔断门板铰链","个",null,"硬塑"]
["1.1.94","大便冲水阀维修","处",null,"含材料、人工"]
["1.1.95","小便冲水阀维修","处",null,"含材料、人工"]
["1.1.96","疏通卫生间下水","处",null,"含材料、人工"]
["1.1.97","水箱支架安装","付",null,"含材料、人工"]
["1.1.98","BV-1.5，电线","m",null,"鑫科"]
["1.1.99","BV-6，电线","m",null,"鑫科"]
["1.1.100","T5/22W，吸顶灯","套",null,"含材料、人工"]
["1.1.101","T5/32W，吸顶灯","套",null,"含材料、人工"]
["1.1.102","20W,日光灯管","根",null,"含材料、人工"]
["1.1.103","36W,日光灯管","根",null,"含材料、人工"]
["1.1.104","DN20，PVC中型电工管","m",null,"含束接、弯头、锁母"]
["1.1.105","三孔插座","个",null,"16A，"]
["1.1.106","PVC线槽","m",null,"TE40×25"]
["1.1.107","De25，PPR等径管套","个",null,"含材料、人工"]
["1.1.108","De20，90度，PPR弯头","个",null,"含材料、人工"]
["1.1.109","De25，PPR截止阀","个",null,"含材料、人工"]
["1.1.110","人工清理沟槽（含油污）","㎡",null,"含材料、人工"]
["1.1.111","人工回填（夯实）土方","m³",null,"含材料、人工"]
["1.1.112","机械回填（松填）土方","m³",null,"含材料、人工"]
["1.1.113","挖掘机进退场费","次",null,"斗容量0.8m3以下"]
["1.1.114","挖掘机进退场费","次",null,"斗容量0.8m3及以上"]
["1.1.115","机械开挖、自卸式汽车配合外运土方","m³",null,"斗容量0.8m3及以上"]
["1.1.116","人工装土、拖拉机外运土方","车",null,"0.8m3"]
["1.1.117","挖土方排水台班","台班",null,"φ110离心清水泵,含人工"]
[1.2,"砌筑工程"]
["1.2.1","拆除120mm厚砖砌体","㎡",null,"含双面粉刷层与垃圾清运费用"]
["1.2.2","拆除370mm厚砖砌体","㎡",null,"含双面粉刷层与垃圾清运费用"]
["1.2.3","砖砌体","m³",null,"利用原有砖体，海螺牌水泥"]
["1.2.4","砖砌体1：2水泥砂浆粉刷增减10mm厚","㎡",null,"中粗沙、海螺牌水泥"]
["1.2.5","天棚水泥砂浆粉刷层20mm厚","㎡",null,"含材料、人工"]
["1.2.6","砖砌体钢丝网铺设","㎡",null,"含材料、人工"]
["1.2.7","120mm厚墙面开孔≤300mm","个",null,"含恢复"]
["1.2.8","370mm厚墙面开洞≤300mm","个",null,"含恢复"]
["1.2.9","砖墙面开关闷盖开孔（100mm×100mm×50mm）"," 个 ",null,"含材料、人工"]
["1.2.10","中粗砂垫层","m³",null,"含材料、人工"]
["1.2.11","细砂垫层","m³",null,"含材料、人工"]
["1.2.12","3.6～8m装饰脚手架","㎡",null,"含材料、人工"]
["1.2.13","8m以上装饰脚手架","㎡",null,"含材料、人工"]
["1.2.14","活动脚手架","副",null,"每副每天"]
[1.3,"道路、附属工程"]
["1.3.1","人工破除钢筋砼道路","m³",null,"含材料、人工"]
["1.3.2","人工挖碎石、片石","m³",null,"含材料、人工"]
["1.3.3","大型挖掘机风镐破砼","小时",null,"斗容量0.8 m3以上"]
["1.3.4","机械挖碎石、片石","m³",null,"含材料、人工"]
["1.3.5","毛石垫层摊铺","m³",null,"含材料、人工"]
["1.3.6","毛石垫层摊铺(利用原有）","m³",null,"厂内运输"]
["1.3.7","级配碎石垫层铺摊","m³",null,"含材料、人工"]
["1.3.8","钢筋制安","kg",null,"含材料、人工"]
["1.3.9","路侧石拆除","m",null,"含清运出厂，自行处理"]
["1.3.10","路侧石安装","m",null,"就地利用原有路侧石，含辅材，护帮砼甲供"]
["1.3.11","面包砖安装","㎡",null,"乙供材，含辅材，≯50mm的水泥沙混合物结合层"]
["1.3.12","破除地面需要安装照明（安全要求）","次",null,"按每处计量，开工-完工计量一次"]
["1.3.13","填黄土、码运（20kg）","袋",null,"含材料、人工、运输"]
["1.3.14","组合式办公桌拆装","套",null,"含搬运"]
["1.3.15","钢丝网围墙(钢管立柱，钢管框）","m",null,"不含基础"]
["1.3.16","PVC围墙(钢管立柱，PVC护栏）","m",null,"不含基础"]
[1.4,"排水工程",null,null,"含材料、人工"]
["1.4.1","有筋承插式涵管φ400×35×2000mm-Ⅱ敷设","m",null,"含材料、人工"]
["1.4.2","有筋承插式涵管φ500×42×2000mm-Ⅱ敷设","m",null,"含材料、人工"]
["1.4.3","UPVC排水管","m",null,"De160，华亚"]
["1.4.4","UPVC排水45度弯头","个",null,"De50，华亚"]
["1.4.5","UPVC排水45度弯头","个",null,"De75，华亚"]
["1.4.6","UPVC排水45度弯头","个",null,"De160，华亚"]
["1.4.7","UPVC排水90度弯头","个",null,"De50，华亚"]
["1.4.8","UPVC排水90度弯头","个",null,"De75，华亚"]
["1.4.9","UPVC排水90度弯头","个",null,"De110，华亚"]
["1.4.10","UPVC排水90度弯头","个",null,"De160，华亚"]
["1.4.11","UPVC排水直接","个",null,{"v":15,"d":"15.00"}]
["1.4.12","UPVC排水直接","个",null,"De110，华亚"]
["1.4.13","UPVC排水直接","个",null,"De160，华亚"]
["1.4.14","UPVC排水45度带检查口弯头","个",null,"De50，华亚"]
["1.4.15","UPVC排水45度带检查口弯头","个",null,"De75，华亚"]
["1.4.16","UPVC排水45度带检查口弯头","个",null,"De110，华亚"]
["1.4.17","UPVC排水45度带检查口弯头","个",null,"De160，华亚"]
["1.4.18","UPVC排水90度带检查口弯头","个",null,"De50，华亚"]
["1.4.19","UPVC排水90度带检查口弯头","个",null,"De75，华亚"]
["1.4.20","UPVC排水90度带检查口弯头","个",null,"De110，华亚"]
["1.4.21","UPVC排水90度带检查口弯头","个",null,"De160，华亚"]
["1.4.22","疏通Φ160mm雨水管","m",null,"含垃圾清运"]
["1.4.23","疏通Φ200mm雨水管","m",null,"含垃圾清运"]
["1.4.24","疏通Φ300mm雨水管","m",null,"含垃圾清运"]
["1.4.25","疏通Φ400mm雨水管","m",null,"含垃圾清运"]
["1.4.26","疏通Φ600mm雨水管","m",null,"含垃圾清运"]
["1.4.27","疏通Φ800mm雨水管","m",null,"含垃圾清运"]
["1.4.28","疏通Φ300mm污水管","m",null,"含垃圾清运"]
["1.4.29","疏通Φ400mm污水管","m",null,"含垃圾清运"]
["1.4.30","疏通Φ600mm污水管","m",null,"含垃圾清运"]
["1.4.31","清理污水检查井(Ф700）","座",null,"综合各种深度、含垃圾清运"]
["1.4.32","清理300×450×1000雨水井","座",null,"含垃圾清运"]
["1.4.33","清理400×600×800污水井","座",null,"含垃圾清运"]
["1.4.34","清理600×450×1100污水井","座",null,"含垃圾清运"]
["1.4.35","清理1500×800×700污水井","座",null,"含垃圾清运"]
["1.4.36","排水沟清淤（200mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.4.37","排水沟清淤（250mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.4.38","排水沟清淤（350mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.4.39","排水沟清淤（400mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.4.40","排水沟清淤（450mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.4.41","排水沟清淤（500mm宽）","m",null,"综合各种深度、含垃圾清运"]
["1.4.42","清理隔油池及窨井内油污","m³",null,"含垃圾清运"]
["1.4.43","疏通φ400mm污水管内油污","m",null,"含垃圾清运"]
["1.4.44","安装铸铁雨水口篦子（300×450）","套",null,"井圈井盖乙供，含安装辅材"]
["1.4.45","安装混凝土雨水口篦子（300×450）","座",null,"井圈井盖乙供，含安装辅材"]
["1.4.46","窨井、沟槽盖板砼浇筑","m³",null,"含砼，模板（砼C20)"]
["1.4.47","安装明沟盖板","㎡",null,"高分子盖板、承重3T, 乙供"]
[1.5,"混凝土工程"]
["1.5.1","砼地面开孔（Φ75mm，深300）","个",null,"含恢复、垃圾外运"]
["1.5.3","砼地面开孔（Φ160mm，深300）","个",null,"含恢复、垃圾外运"]
["1.5.4","砼地面开孔（Φ200mm，深300）","个",null,"含恢复、垃圾外运"]
["1.5.5","机械切缝并凿除砼地面（宽20~50mm,50mm深）","m",null,"含垃圾外运"]
["1.5.6","机械切缝并凿除砼地面（宽50~100mm,50mm深）","m",null,"含垃圾外运"]
["1.5.7","机械切缝并凿除砼地面（宽100~200mm,50mm深）","m",null,"含垃圾外运"]
["1.5.8","机械切缝并凿除砼地面（宽200~300mm,50mm深）","m",null,"含垃圾外运"]
["1.5.9","机械切缝并凿除砼地面（宽20~50mm,10mm深）","m",null,"含垃圾外运"]
["1.5.10","机械切缝并凿除砼地面（宽50~100mm,10mm深）","m",null,"含垃圾外运"]
["1.5.11","机械切缝并凿除砼地面（宽100~200mm,10mm深）","m",null,"含垃圾外运"]
["1.5.12","机械切缝并凿除砼地面（宽200~300mm,10mm深）","m",null,"含垃圾外运"]
["1.5.13","机械切缝并凿除砼地面（宽50~100mm,250mm深）","m",null,"含垃圾外运"]
["1.5.14","机械切缝并凿除砼地面（宽100~200mm,250mm深）","m",null,"含垃圾外运"]
["1.5.15","机械切缝并凿除砼地面（宽200~300mm,250mm深）","m",null,"含垃圾外运"]
["1.5.16","机械切缝并凿除砼地面（宽20~50mm,250mm深）","m",null,"含垃圾外运"]
["1.5.17","机械切缝并凿除砼地面（宽50~100mm,350mm深）","m",null,"含垃圾外运"]
["1.5.18","机械切缝并凿除砼地面（宽100~200mm,350mm深）","m",null,"含垃圾外运"]
["1.5.19","机械切缝并凿除砼地面（宽200~300mm,350mm深）","m",null,"含垃圾外运"]
["1.5.20","机械切缝并凿除砼地面（宽20~50mm,350mm深）","m",null,"含垃圾外运"]
["1.5.21","机械切缝并凿除砼地面（宽50~100mm,150mm深）","m",null,"含垃圾外运"]
["1.5.22","机械切缝并凿除砼地面（宽100~200mm,150mm深）","m",null,"含垃圾外运"]
["1.5.23","机械切缝并凿除砼地面（宽200~300mm,150mm深）","m",null,"含垃圾外运"]
["1.5.24","机械切缝并凿除砼地面（宽20~50mm,150mm深）","m",null,"含垃圾外运"]
["1.5.25","机械切缝并凿除砼地面（宽50~100mm,120mm深）","m",null,"含垃圾外运"]
["1.5.26","机械切缝并凿除砼地面（宽100~200mm,120mm深）","m",null,"含垃圾外运"]
["1.5.27","机械切缝并凿除砼地面（宽200~300mm,120mm深）","m",null,"含垃圾外运"]
["1.5.28","机械切缝并凿除砼地面（宽20~50mm,120mm深）","m",null,"含垃圾外运"]
["1.5.29","机械切缝并凿除砼地面（宽50~100mm,200mm深）","m",null,"含垃圾外运"]
["1.5.30","机械切缝并凿除砼地面（宽100~200mm,200mm深）","m",null,"含垃圾外运"]
["1.5.31","机械切缝并凿除砼地面（宽200~300mm,200mm深）","m",null,"含垃圾外运"]
["1.5.32","机械切缝并凿除砼地面（宽20~50mm,200mm深）","m",null,"含垃圾外运"]
["1.5.33","机械切缝并凿除砼地面（宽50~100mm,100mm深）","m",null,"含垃圾外运"]
["1.5.34","机械切缝并凿除砼地面（宽100~200mm,100mm深）","m",null,"含垃圾外运"]
["1.5.35","机械切缝并凿除砼地面（宽200~300mm,100mm深）","m",null,"含垃圾外运"]
["1.5.36","机械切缝并凿除砼地面（宽20~50mm,100mm深）","m",null,"含垃圾外运"]
["1.5.37","高分子踢脚线","m",null,"含材料、人工"]
["1.5.38","免漆护墙板墙面","㎡",null,"含材料、人工"]
["1.5.39","顶棚、墙面原有风机孔洞吊模封堵","个",null,"含材料、人工"]
["1.5.40","顶棚、墙面原有排烟、通风管道洞\n孔封堵","个",null,"含材料、人工"]
["1.5.41","普通硅酸盐水泥","袋"]
["1.5.42","C15地坪浇筑","m³",null,"砼自拌"]
["1.5.43","C20地坪浇筑","m³",null,"砼自拌"]
["1.5.44","C30地坪浇筑","m³",null,"砼自拌"]
["1.5.45","人工浇筑钢筋砼基础","m³",null,"不含钢筋制安，"]
["1.5.46","人工浇筑钢筋砼梁、板、柱","m³",null,"不含钢筋制安，"]
["1.5.47","砼二次倒运","m³",null,"运距10米以外"]
["1.5.48","二次砼灌浆（自拌砼）","m³",null,"自拌微膨胀混凝土 "]
["1.5.49","钢筋制安","kg",null,"马钢或国内大型钢厂产品"]
[1.6,"金属结构、其它工程"]
["1.6.1","双层彩钢板墙面开孔φ160mm以下圆孔","个",null,"含收边费用"]
["1.6.2","双层彩钢板墙面开孔φ300mm以下圆孔","个",null,"含收边费用"]
["1.6.3","彩钢板墙体开洞1.2×1.2以内","个",null,"含收边、垃圾清运费"]
["1.6.4","双层彩钢板面收边（镀锌，展开宽度≤500mm）","m",null,"含材料、人工"]
["1.6.5","门洞口单层彩板包边","m",null,"含材料、人工"]
["1.6.6","100m厚EPS板镀锌铁皮包边","m",null,"含材料、人工"]
["1.6.7","镀锌铁皮包边（厚3mm，宽3cm，含打孔及辅材）","m",null,"含材料、人工"]
["1.6.8","Φ110防撞柱安装（插入地面式安装，含四周灌浆）","个",null,"含材料、人工"]
["1.6.9","拉结筋植筋胶植筋（Φ8 L=0.95m)","根",null,"含材料、人工"]
["1.6.10","植筋胶植筋（Φ6，均长0.5m）","根",null,"含材料、人工"]
["1.6.11","钢板网制安(80×50×5)","㎡",null,"含材料、人工"]
["1.6.12","水管保温DN15","m",null,"含材料、人工"]
["1.6.13","水管保温DN20","m",null,"橡塑保温"]
["1.6.14","水管保温DN32","m",null,"橡塑保温"]
["1.6.15","水包绑扎保温","个",null,"含材料、人工"]
["1.6.16","卷帘窗帘","㎡",null,"含材料、人工"]
["1.6.17","厂房卷帘门拆卸矫正、更换部分配件","m2",null,"含材料、人工"]
["1.6.18","厂房卷帘门更换电机","组",null,"含材料、人工"]
["1.6.19","卷帘门轨槽","m",null,"含材料、人工"]
["1.6.20","门禁系统电机","套",null,"含材料、人工"]
["1.6.21","不锈钢包门头横梁","㎡",null,"含材料、人工"]
["1.6.22","12mm厚钢化玻璃门","㎡",null,"含材料、人工"]
["1.6.23","PVC门边条","m",null,"含材料、人工"]
["1.6.24","铝门边条","m",null,"含材料、人工"]
["1.6.25","不锈钢包门边框","m",null,"含材料、人工"]
["1.6.26","沙袋","袋",null,"27.5公斤一袋"]
["1.6.27","沙袋","袋",null,"25.0公斤一袋"]
["1.6.28","沙袋","袋",null,"18.0公斤一袋"]
["二","装饰",null,null,"含材料、人工"]
[2.1,"油漆、涂料、裱糊工程"]
["2.1.1","铁门围栏刷油漆（两遍）","m2",null,"含材料、人工"]
["2.1.2","金属面防锈漆（一遍）","m2",null,"含除锈、材料、人工"]
["2.1.3","金属面面漆（两遍）","m2",null,"含材料、人工"]
["2.1.4","木面油漆（两遍）","m2",null,"含材料、人工"]
["2.1.5","钢丝网围栏油漆（两遍）","m2",null,"含除锈、一底二面"]
["2.1.6","木扶手油漆（两遍）","m",null,"含油灰打底"]
["2.1.7","钢柱喷字","个",null,"字高30cm以内"]
["2.1.8","铲除原有顶面涂料","㎡",null,"含垃圾清运费用"]
["2.1.9","铲除原有墙面涂料","㎡",null,"含垃圾清运费用"]
["2.1.10","刷内墙乳胶漆一底两面","㎡",null,"含材料、人工"]
["2.1.11","刷墙面防霉涂料","㎡",null,"含材料、人工"]
["2.1.12","刷顶面防霉涂料","㎡",null,"含材料、人工"]
["2.1.13","安装硅钙板吊顶","㎡",null,"含材料、人工"]
["2.1.14","轻钢龙骨防火石膏板吊顶","㎡",null,"含材料、人工"]
["2.1.15","轻钢龙骨硅钙板吊顶更换","㎡",null,"含材料、人工"]
["2.1.16","轻钢龙骨纸面防潮石膏板隔墙双面石膏板","㎡",null,"含材料、人工"]
["2.1.17","轻钢龙骨防火石膏板吊顶","㎡",null,"含材料、人工"]
["2.1.18","铝塑板包柱及横梁","㎡",null,"含材料、人工"]
[2.2,"楼地面、墙、柱面装饰工程",null,null,"含材料、人工"]
["2.2.1","铲除原有地面瓷砖","㎡",null,"含垃圾清运费用"]
["2.2.2","铲除原有墙面瓷砖","㎡",null,"含垃圾清运费用"]
["2.2.3","铲除原有瓷砖踢脚线","m",null,"含垃圾清运费用"]
["2.2.6","水泥砂浆贴地面砖","㎡",null,"含材料、人工"]
["2.2.7","水泥砂浆贴墙面砖","㎡",null,"含材料、人工"]
["2.2.8","水泥砂浆贴门槛石","㎡",null,"中国黑、厚度10mm以上"]
["2.2.9","贴120mm高大理石踢脚线","m",null,"中国黑、厚度10mm以上"]
[2.3,"门窗工程"]
["2.3.1","安装58型材PVC半玻平开门","㎡",null,"海螺型材、5mm单玻璃"]
["2.3.2","安装58型材PVC全玻平开门","㎡",null,"海螺型材、5mm单玻璃"]
["2.3.3","安装58型材PVC全板平开门","㎡",null,"海螺型材"]
["2.3.4","安装60型材PVC半玻推拉门","㎡",null,"海螺型材、5mm单玻璃"]
["2.3.5","安装防盗门","㎡",null,"门锁及配件"]
["2.3.6","安装防盗门","㎡",null,"贝斯特，含门锁及配件"]
["2.3.7","安装防火门","㎡",null,"甲级，含门锁及配件"]
["2.3.8","安装彩铝拉门","㎡"]
["2.3.9","安装10mm厚钢化玻璃门","㎡",null,"不含主材"]
["2.3.10","安装12mm厚钢化玻璃门","㎡",null,"不含主材"]
["2.3.11","安装58型材PVC固定窗","㎡",null,"海螺型材、5mm单玻璃"]
["2.3.12","安装60型PVC平开窗","㎡",null,"海螺型材、5mm单玻璃，含窗扇及配件，不含窗框"]
["2.3.13","安装88型材推拉窗","㎡",null,"海螺型材、5mm单玻璃"]
["2.3.14","安装5mm厚门、窗玻璃","㎡",null,"含材料、人工"]
["2.3.15","安装玻璃地弹门拉手450mm长","副",null,"含材料、人工"]
["2.3.16","安装玻璃地弹门拉手600mm长","副",null,"含材料、人工"]
["2.3.17","安装玻璃门地弹簧","套",null,"含材料、人工"]
["2.3.18","安装玻璃门锁","把",null,"半圆内侧带保险"]
["2.3.19","安装钢化玻璃门夹","只",null,"含材料、人工"]
["2.3.20","安装GMT玻璃门导轨","m",null,"含材料、人工"]
["2.3.21","安装玻璃门门吸","套",null,"含材料、人工"]
["2.3.22","安装玻璃门锁","把",null,"含材料、人工"]
["2.3.23","安装玻璃门锁","把",null,"含材料、人工"]
["2.3.24","600mm不锈钢推拉门把手固定维修","个",null,"含材料、人工"]
["2.3.25","安装PVC窗把手","只",null,"含材料、人工"]
["2.3.26","安装PVC窗铝合金把手","只",null,"含材料、人工"]
["2.3.27","安装T型PVC锁","把",null,"含材料、人工"]
["2.3.28","安装PVC门铰链","只",null,"含材料、人工"]
["2.3.29","安装PVC门上扣","只",null,"含材料、人工"]
["2.3.30","安装PVC窗月牙锁","只",null,"含材料、人工"]
["2.3.31","安装PVC窗滑轮","只",null,"含材料、人工"]
["2.3.32","安装PVC窗折叠杆","只",null,"含材料、人工"]
["2.3.33","安装PVC平开窗拉手","把",null,"含材料、人工"]
["2.3.34","安装PVC窗铝滑轨","m",null,"含材料、人工"]
["2.3.35","安装PVC窗毛条","m",null,"含材料、人工"]
["2.3.36","安装PVC窗橡胶压条","m",null,"含材料、人工"]
["2.3.37","安装PVC窗胶条","m",null,"含材料、人工"]
["2.3.38","PVC纱窗换纱","㎡",null,"含材料、人工"]
["2.3.39","PVC纱窗换纱","㎡",null,"仅换纱不含框料，含压条"]
["2.3.40","安装不锈钢纱窗","㎡",null,"含材料、人工"]
["2.3.41","安装木门防盗锁芯","把",null,"含材料、人工"]
["2.3.42","安装木门执手锁","把",null,"含材料、人工"]
["2.3.43","安装木门执手锁","把",null,"含材料、人工"]
["2.3.44","木门执手锁维修","把",null,"含材料、人工"]
["2.3.45","安装PVC门球形锁","把",null,"含材料、人工"]
["2.3.46","安装PVC门执手锁","把",null,"含材料、人工"]
["2.3.47","安装PVC门执手锁芯","把",null,"含材料、人工"]
["2.3.48","安装PVC门加长型门锁","把",null,"含材料、人工"]
["2.3.49","安装PVC门加长型门锁芯","把",null,"含材料、人工"]
["2.3.50","安装防盗门锁","把",null,"含材料、人工"]
["2.3.51","安装防火门锁","把",null,"含材料、人工"]
["2.3.52","安装防盗门把手","只",null,"含材料、人工"]
["2.3.53","安装防盗门执手锁锁芯","把",null,"含材料、人工"]
["2.3.54","安装闭门器062型","套",null,"含材料、人工"]
["2.3.55","安装80mm长普通插销","套",null,"含材料、人工"]
["2.3.56","安装120mm长不锈钢插销","套",null,"含材料、人工"]
["2.3.57","安装200mm长不锈钢插销","套",null,"含材料、人工"]
["2.3.58","安装300mm长不锈钢插销","套",null,"含材料、人工"]
["2.3.59","不锈钢网制安","㎡",null,"含材料、人工"]
["2.3.60","不锈钢防鼠板门制安","㎡",null,"含材料、人工"]
["2.3.61","贴窗纸","㎡",null,"含材料、人工"]
[2.4,"卫生间工程",null,null,"含材料、人工"]
["2.4.1","台面上脸盆","套",null,"含安装辅材"]
["2.4.2","脸盆用单把水龙头","只",null,"含安装辅材"]
["2.4.3","S弯下水","只",null,"含安装辅材"]
["2.4.4","高压软管","根",null,"含安装辅材"]
["2.4.5","三角阀","只",null,"含安装辅材"]
["2.4.6","立柱式脸盆","套",null,"含安装辅材"]
["2.4.7","拖把池","套",null,"含安装辅材"]
["2.4.8","拖把池龙头","套",null,"含安装辅材"]
["2.4.9","安装大便器按钮式冲洗阀","只",null,"含材料、人工"]
["2.4.10","安装大便器压杆式冲洗阀","只",null,"含材料、人工"]
["2.4.11","安装洗面盆双联龙头","只",null,"含材料、人工"]
["2.4.12","安装洗面盆双联龙头","只",null,"含材料、人工"]
["2.4.13","安装拖布池加长型单开水龙头","只",null,"含材料、人工"]
["2.4.14","安装拖布池单开普通水龙头","只",null,"含材料、人工"]
["2.4.15","安装立式弯管水龙头 ","只",null,"含材料、人工"]
["2.4.16","安装面盆下水配件","套",null,"含材料、人工"]
["2.4.17","安装水龙头给水软管","根",null,"含材料、人工"]
["2.4.18","安装水龙头加长型给水软管(L≥0.5m)","根",null,"含材料、人工"]
["2.4.19","安装洗面盆S形不锈钢下水配件","套",null,"含材料、人工"]
["2.4.20","安装洗面盆塑料排水软管","套",null,"含材料、人工"]
["2.4.21","安装卫生间隔断门板（门板尺寸1700×600）","㎡",null,"含材料、人工"]
["2.4.22","安装卫生间隔断门板锁具","个",null,"硬塑角码、地脚配件等"]
["2.4.23","安装卫生间隔断门板铰链","个",null,"不锈钢"]
["2.4.24","安装卫生间隔断门板锁具","个",null,"不锈钢"]
["2.4.25","安装小便池挡板","块",null,"含材料、人工"]
["2.4.26","安装镜子","㎡",null,"含材料、人工"]
["2.4.27","聚氨酯防水层（两道）","㎡",null,"含材料、人工"]
["2.4.28","卫生间防水（SQ厚2.5mm）","㎡",null,"含材料、人工"]
["2.4.29","PVC扣板开孔（300×300）","个",null,"含材料、人工"]
["2.4.30","不锈钢地漏（De50）","个",null,"含材料、人工"]
["2.4.31","不锈钢地漏（De75）","个",null,"含材料、人工"]
["2.4.32","不锈钢地漏（De100）","个",null,"含材料、人工"]
["2.4.33","淋浴花洒拆换","套",null,"含材料、人工"]
["2.4.34","不锈钢角架安装","只",null,"含材料、人工"]
["2.4.35","不锈钢挂衣架安装","只",null,"含材料、人工"]
["2.4.36","蹲坑成套水箱安装","套",null,"含材料、人工"]
["2.4.37","安装衣帽钩","个",null,"含材料、人工"]
["三","安装工程",null,null,"含材料、人工"]
[3.1,"电气工程",null,null,"含材料、人工"]
["3.1.2","BV-2.5，电线","m",null,"鑫科"]
["3.1.3","BV-4，电线","m",null,"鑫科"]
["3.1.4","BV-10，电线","m",null,"鑫科"]
["3.1.5","BV-16，电线","m",null,"鑫科"]
["3.1.6","BV-25，电线","m",null,"鑫科"]
["3.1.7","3×2.5m㎡护套线敷设","m",null,"鑫科"]
["3.1.8","2×14W，标准型电子镇流器（一拖二）","套",null,"含材料、人工"]
["3.1.9","2×28W，标准型电子镇流器（一拖二）","套",null,"含材料、人工"]
["3.1.10","3×14W，标准型电子镇流器（一拖三）","套",null,"含材料、人工"]
["3.1.11","3×28W，标准型电子镇流器（一拖三）","套",null,"含材料、人工"]
["3.1.12","暗装配电箱壳体","套",null,"8位，含导轨、零排、接地排，正泰"]
["3.1.13","暗装配电箱壳体","套",null,"12位，含导轨、零排、接地排，正泰"]
["3.1.14","暗装配电箱壳体","套",null,"24位，含导轨、零排、接地排，正泰"]
["3.1.15","明装配电箱壳体","套",null,"8位，含导轨、零排、接地排，正泰"]
["3.1.16","明装配电箱壳体","套",null,"12位，含导轨、零排、接地排，正泰"]
["3.1.17","明装配电箱壳体","套",null,"24位，含导轨、零排、接地排，正泰"]
["3.1.18","T5/28W，吸顶灯","套"]
["3.1.19","T5/40W，吸顶灯","套"]
["3.1.20","消防应急标志灯","套",null,"PAK-Y01-101~106，应急时间≥90min，"]
["3.1.21","消防应急照明灯","套",null,"PAK-Y01-208AX，应急时间≥90min，"]
["3.1.22","不锈钢防雨配电箱","套"]
["3.1.23","3*50YJV-22电缆线","m"]
["3.1.24","DN75，PVC中型电工管","m"]
["3.1.25","200*1200mmLED办公吊线灯","套"]
["3.1.26","600*600mmLED平板灯","套"]
["3.1.27","YJV5*2.5mm2电缆线","m"]
["3.1.28","YJV5*10电缆线","m"]
["3.1.29","3P50A空开","个"]
["3.1.30","4P63A保护器","个"]
["3.1.31","4P100A保护器","个"]
["3.1.32","4P50A漏电保护器","个"]
["3.1.33","3P漏电保护器50A","个"]
["3.1.34","3P漏电保护器40A","个"]
["3.1.35","2P漏电保护器25A","个"]
["3.1.36","2P32A保护器","个"]
["3.1.37","2P保护器25A","个"]
["3.1.38","1P保护器20A","个"]
["3.1.39","1P保护器16A","个"]
["3.1.40","暗盒盖板","个"]
["3.1.41","3×14W，T5，嵌入式格栅灯","套",null,"含材料、人工"]
["3.1.42","3×28W，T5，嵌入式格栅灯","套",null,"含材料、人工"]
["3.1.43","3×36W，T5，嵌入式格栅灯","套",null,"含材料、人工"]
["3.1.44","18W,日光灯管","根",null,"含材料、人工"]
["3.1.45","24W,日光灯管","根",null,"含材料、人工"]
["3.1.46","40W,日光灯管","根",null,"含材料、人工"]
["3.1.47","32W环形灯管","套",null,"含材料、人工"]
["3.1.48","25W螺旋节能灯管","套",null,"含材料、人工"]
["3.1.49","DN16，PVC中型电工管","m",null,"含束接、弯头、锁母"]
["3.1.50","DN25，PVC中型电工管","m",null,"含束接、弯头、锁母"]
["3.1.51","DN32，PVC中型电工管","m",null,"含束接、弯头、锁母"]
["3.1.52","DN40，PVC中型电工管","m",null,"含束接、弯头、锁母"]
["3.1.53","DN50，PVC中型电工管","m",null,"含束接、弯头、锁母"]
["3.1.54","DN15，PVC接线盒","个",null,"含材料、人工"]
["3.1.55","DN20，PVC接线盒","个",null,"含材料、人工"]
["3.1.56","DN25，PVC接线盒","个",null,"含材料、人工"]
["3.1.57","单极翘板开关","个",null,"10A，"]
["3.1.58","双极翘板开关","个",null,"10A，"]
["3.1.59","三极翘板开关","个",null,"10A，"]
["3.1.60","四极翘板开关","个",null,"10A，"]
["3.1.61","安装声控开关","只"]
["3.1.62","五孔插座","个",null,"10A，"]
["3.1.63","三孔插座16A（充电桩专用）","个"]
["3.1.64","明盒","个",null,"86型，"]
["3.1.65","暗盒","个",null,"86型，"]
["3.1.66","PVC角线槽","m",null,"TC40*40，"]
["3.1.67","PVC地面线槽","m",null,"TC50*15"]
["3.1.68","PVC地面线槽","m",null,"TC75*18"]
["3.1.69","PVC线槽","m",null,"TE25*15"]
["3.1.70","PVC线槽","m",null,"TE40*20"]
["3.1.71","PVC线槽","m",null,"TE60*25"]
["3.1.72","PVC线槽 ","m",null,"TE85×40"]
["3.1.73","不锈钢地面弧线槽100mm宽","m",null,"含材料、人工"]
["3.1.74","不锈钢弧形地线槽50mm宽","m",null,"含材料、人工"]
["3.1.75","金属线槽安装100×50","m",null,"含材料、人工"]
["3.1.76","半圆形铝合金线槽","m",null,"60*20"]
["3.1.77","半圆形铝合金线槽","m",null,"50*15"]
["3.1.78","安装8回路电箱盖","个",null,"含材料、人工"]
["3.1.79","安装10回路电箱盖","个",null,"含材料、人工"]
["3.1.80","安装15回路电箱盖","个",null,"含材料、人工"]
["3.1.81","安装18回路电箱盖","个",null,"含材料、人工"]
["3.1.82","安装24回路电箱盖","个",null,"含材料、人工"]
["3.1.83","排气扇","个",null,"含材料、人工"]
[3.2,"给水工程",null,null,"含材料、人工"]
["3.2.1","De20，PPR等径管套","个",null,"含材料、人工"]
["3.2.2","De32，PPR等径管套","个",null,"含材料、人工"]
["3.2.3","De25，90度，PPR弯头","个",null,"含材料、人工"]
["3.2.4","De32，90度，PPR弯头","个",null,"含材料、人工"]
["3.2.5","De20，45度，PPR弯头","个",null,"含材料、人工"]
["3.2.6","De25，45度，PPR弯头","个",null,"含材料、人工"]
["3.2.7","De32，45度，PPR弯头","个",null,"含材料、人工"]
["3.2.8","De20，PPR等径三通","个",null,"含材料、人工"]
["3.2.9","De25，PPR等径三通","个",null,"含材料、人工"]
["3.2.10","De32，PPR等径三通","个",null,"含材料、人工"]
["3.2.11","De50，PPR等径三通","个",null,"含材料、人工"]
["3.2.12","De63，PPR等径三通","个",null,"含材料、人工"]
["3.2.13","De75，PPR等径三通","个",null,"含材料、人工"]
["3.2.14","De20，PPR截止阀","个",null,"含材料、人工"]
["3.2.15","De32，PPR截止阀","个",null,"含材料、人工"]
["3.2.16","De50，PPR截止阀","个",null,"含材料、人工"]
["四","钢结构",null,null,"含材料、人工"]
[4.1,"预埋铁件制作安装","kg",null,"含材料、人工"]
["4.1.1","预埋高强螺栓制作安装","kg",null,"含材料、人工"]
["4.1.2","膨胀螺栓安装φ6-φ10","个",null,"含材料、人工"]
["4.1.3","膨胀螺栓安装φ12-φ16","个",null,"含材料、人工"]
["4.1.4","膨胀螺栓安装φ18-φ22","个",null,"含材料、人工"]
["4.1.5","膨胀螺栓安装φ24-φ28","个",null,"含材料、人工"]
["4.1.6","膨胀螺栓安装φ28-φ32","个",null,"含材料、人工"]
["4.1.7","Φ14mm化学螺栓制安","套",null,"含材料、人工"]
["4.1.8","Φ20mm化学螺栓制安","套",null,"含材料、人工"]
["4.1.9","彩钢瓦拆除","m2",null,"含材料、人工"]
["4.1.10","彩钢瓦恢复，厚0.5mm","m2",null,"含材料、人工"]
["4.1.11","钢梁柱拆除","t",null,"含材料、人工"]
["4.1.12","钢檩条及钢柱恢复","t",null,"含材料、人工"]
["4.1.13","塑钢窗的拆除","m2",null,"含材料、人工"]
["4.1.14","厂房推拉门插销制安","个",null,"含材料、人工"]
["4.1.15","厂房推拉门夹芯板铆钉制安","m2",null,"含材料、人工"]
["4.1.16","墙面彩钢瓦整形修复","m2",null,"含材料、人工"]
["4.1.17","电缆地沟盖板（铁制：1.1m*0.6m)","块",null,"含材料、人工"]
["4.1.18","制作安装60型材PVC固定窗","㎡",null,"海螺型材"]
["4.1.19","制作安装88型材推拉窗(带纱窗)","㎡",null,"海螺型材"]
["4.1.20","制作安装88型材推拉窗(带纱窗)","㎡",null,"海螺型材"]
["4.1.21","制作安装PVC纱窗","㎡",null,"单扇不足1m2按1m2计"]
["4.1.22","制作安装PVC纱门","扇",null,"含材料、人工"]
["4.1.23","制作安装58型材PVC半玻平开门","㎡",null,"海螺型材"]
["4.1.24","制作安装58型材PVC全玻平开门","㎡",null,"海螺型材"]
["4.1.25","制作安装58型材PVC镶板隔断","㎡",null,"立杆间距1.2M以内"]
["4.1.26","制作安装铝合金半玻平开门2.0mm","㎡",null,"含材料、人工"]
["4.1.27","制作安装铝合金全板平开门2.0mm","㎡",null,"含材料、人工"]
["4.1.28","制作安装铝合金推拉窗1.4mm","㎡",null,"含材料、人工"]
["4.1.29","制作安装铝合金固定窗1.4mm","㎡",null,"含材料、人工"]
["4.1.30","制作安装75mm岩棉墙体","㎡",null,"含包边，辅材、内外板0.5mm"]
["4.1.31","制作安装75mm岩棉板门","㎡",null,"含包边，辅材、内外板0.5mm"]
["4.1.32","制作安装75mm岩棉瓦楞屋面板","㎡",null,"含包边，辅材、内外板0.5mm"]
["4.1.33","制作安装50mm岩棉墙体","㎡",null,"含包边，辅材、内外板0.5mm"]
["4.1.34","制作安装50mm岩棉板门","㎡",null,"含包边，辅材、内外板0.5mm"]
["4.1.35","制作安装50mm岩棉瓦楞屋面板","㎡",null,"含包边，辅材、内外板0.5mm"]
["4.1.36","制作安装1.05M高不锈钢栏杆","m",null,"含材料、人工"]
["4.1.37","不锈钢栏杆维修","m",null,"综合各种管径，含焊接"]
["4.1.38","制作安装δ=0.45mm泛水板","㎡",null,"展开宽度≤300mm"]
["4.1.39","制作安装δ=0.45mm泛水板","㎡",null,"展开宽度≤500mm"]
["4.1.40","制作安装δ=0.50mm屋面板","㎡",null,"镀锌彩板"]
["4.1.41","制作安装δ=0.5mm墙面板","㎡",null,"镀锌彩板、板宽1M以内"]
["4.1.42","轻钢龙骨双面石膏板墙制安（可耐福板）","m2",null,"含材料、人工"]
["4.1.43","轻钢龙骨单面石膏板墙制安（可耐福板）","m2",null,"含材料、人工"]
["4.1.44","轻钢龙骨铝塑板天棚制安","m2",null,"含材料、人工"]
["4.1.45","轻钢龙骨铝合金扣板制安","m2",null,"含材料、人工"]
["4.1.46","木龙骨PVC扣板天棚制安","m2",null,"含材料、人工"]
["4.1.47","角钢框、钢丝网隔断制安","m2",null,"含材料、人工"]
["4.1.48","5mm厚平板玻璃制安","m2",null,"含材料、人工"]
["4.1.49","打玻璃胶","m",null,"含材料、人工"]
["4.1.50","打结构胶","m",null,"含材料、人工"]
["4.1.51","打膨胀剂","m",null,"含材料、人工"]
["4.1.52","3㎜聚酯SBS防水卷材铺设","m2",null,"含材料、人工"]
["4.1.53","4mm厚聚酯胎SBS防水层铺设","m2",null,"含材料、人工"]
["4.1.54","JS高分子复合防水涂料1.2厚","m2",null,"含材料、人工"]
["4.1.55","堵漏王补漏","袋",null,"含材料、人工"]
["4.1.56","防水浆料","kg",null,"含材料、人工"]
["4.1.57","制作彩钢雨棚","m2",null,"不含柱"]
["4.1.58","铝合金网状防盗窗制安","m2",null,"含材料、人工"]
["4.1.59","不锈钢防盗窗制安","m2",null,"含材料、人工"]
["4.1.60","不锈钢防盗窗制安","m2",null,"含开小门"]
["4.1.61","不锈钢包边（1mm厚304，L10cm*10cm宽）","m",null,"含木工板打底"]
["4.1.62","方管防盗窗制安（含底漆、面漆）","m2",null,"含材料、人工"]
["4.1.63","厂房卷帘门拆卸矫正、更换部分配件","m2",null,"含材料、人工"]
["4.1.64","厂房卷帘门更换电机","组",null,"含材料、人工"]
["4.1.65","铝合金门矫正、维修","扇",null,"含材料、人工"]
["4.1.66","厂房天沟虹吸接头处漏雨维修","处",null,"湾头处脱焊修复"]
["4.1.67","非金属墙面渗水维修","处",null,"含材料、人工"]
["4.1.68","彩钢瓦屋面漏水维修","处",null,"屋面打结构胶"]
["4.1.69","金属面防锈漆（一遍）","m2",null,"含除锈、材料、人工"]
["4.1.70","金属面面漆（两遍）","m2",null,"含材料、人工"]
["4.1.71","钢栏杆油漆（两遍）","m",null,"含除锈、一底二面"]
["4.1.72","吊机 25T","台班"]
["4.1.73","随车吊 8T","台班"]
["4.1.74","管道疏通车 20T","台班"]
["4.1.75","登高车","台班"]
["4.1.76","不锈钢室外充电箱","套"]
["4.1.77","消防软管卷盘","盘"]
["4.1.78","复合地板","m2"]
["4.1.79","地板革","m2"]
["4.1.80","鹅卵石","t"]
["4.1.81","消防箱门","扇"]
["4.1.82","消防箱","套"]
["4.1.83","18厘板","m2"]
["4.1.84","1P32A漏电保护器","个"]
["4.1.85","地面标识标线","m"]
["4.1.86","集装箱租赁（3*6m）","天",null,"含挂壁空调一台"]
["4.1.87","集装箱租赁（3*6m）","天",null,"不含空调"]
["4.1.88","集装箱租赁（6*6m）","天",null,"含挂壁空调两台"]
["4.1.89","集装箱租赁（6*6m）","天",null,"不含空调"]
["4.1.90"]
["4.1.91"]
["4.1.94","UPVC排水管300","m"]
["4.1.95","5+9A+5钢化中空玻璃","m2",null,"含材料、人工"]
["4.1.96","不锈钢水槽","套",null,"含材料、人工"]
["4.1.97","不锈钢外丝直接","个",null,"含材料、人工"]
["4.1.98","304不锈钢三通","个",null,"含材料、人工"]
["4.1.99","UPVC50*20大小头","个",null,"含材料、人工"]
["4.1.100","UPVC75*50大小头","个",null,"含材料、人工"]
["4.1.101","UPVC110*75大小头","个",null,"含材料、人工"]
["4.1.102","UPVC110雨水漏斗","个",null,"含材料、人工"]
["4.1.103","仿真贴纸","m2",null,"含材料、人工"]
["4.1.104","De20PE给水管","m",null,"含材料、人工"]
["4.1.105","De32PPR给水管","m",null,"含材料、人工"]
["4.1.106","De20PPR给水管","m",null,"含材料、人工"]
["4.1.107","给水增压泵","台",null,"含材料、人工"]
["4.1.108","防水石塑地板","m2",null,"含材料、人工"]
["4.1.109","轻钢龙骨","m2",null,"含材料、人工"]
["4.1.110","隔断门板不锈钢拉手","个",null,"含材料、人工"]
["4.1.111","淋浴隔断铝合金拉杆","m",null,"含材料、人工"]
["4.1.112","实木生态板淋浴隔断","m2",null,"含材料、人工"]
["4.1.113","300mm宽不锈钢水沟盖板","m",null,"含材料、人工"]
["4.1.114","软包背景墙板","m2",null,"含材料、人工"]
["4.1.115","安装75mm岩棉墙体辅材","m2",null,"含材料、人工"]
["4.1.116","脚手架出入场运输费","项"]
["合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}